*************************** START ****************************

START TIME: 202308081522

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 263.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 331.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 456.8 kbit/s)...

Hash of data verified.
Wrote 792000 bytes (450430 compressed) at 0x00010000 in 8.4 seconds (effective 752.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202308081526

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 264.5 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 334.7 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 456.2 kbit/s)...

Hash of data verified.
Wrote 792000 bytes (450430 compressed) at 0x00010000 in 8.5 seconds (effective 749.6 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202308081535

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 264.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 332.8 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 457.3 kbit/s)...

Hash of data verified.
Wrote 792048 bytes (450450 compressed) at 0x00010000 in 8.5 seconds (effective 747.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



