*************************** START ****************************

START TIME: 202308081522

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 263.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 331.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 456.8 kbit/s)...

Hash of data verified.
Wrote 792000 bytes (450430 compressed) at 0x00010000 in 8.4 seconds (effective 752.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202308081526

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 264.5 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 334.7 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 456.2 kbit/s)...

Hash of data verified.
Wrote 792000 bytes (450430 compressed) at 0x00010000 in 8.5 seconds (effective 749.6 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202308081535

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 264.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 332.8 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 457.3 kbit/s)...

Hash of data verified.
Wrote 792048 bytes (450450 compressed) at 0x00010000 in 8.5 seconds (effective 747.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202308081541

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 264.5 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 337.1 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 457.9 kbit/s)...

Hash of data verified.
Wrote 793808 bytes (451524 compressed) at 0x00010000 in 8.5 seconds (effective 745.2 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202308081546

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 268.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 336.1 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 459.3 kbit/s)...

*************************** START ****************************

START TIME: 202308081546

CONNECT BAUD: 115200
serial port open error
COM:COM3
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202308081547

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 255.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 538.3 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 872.2 kbit/s)...

Hash of data verified.
Wrote 793808 bytes (451524 compressed) at 0x00010000 in 8.4 seconds (effective 756.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202308101449

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 266.5 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 339.8 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 462.5 kbit/s)...

Hash of data verified.
Wrote 793808 bytes (451524 compressed) at 0x00010000 in 8.6 seconds (effective 740.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202308101611

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 267.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 338.6 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 457.5 kbit/s)...

Hash of data verified.
Wrote 793808 bytes (451524 compressed) at 0x00010000 in 8.6 seconds (effective 742.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202308101844

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 266.1 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 341.2 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 451.2 kbit/s)...

Hash of data verified.
Wrote 859744 bytes (471855 compressed) at 0x00010000 in 9.1 seconds (effective 758.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202308110939

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x55213ebc
mac h: 0xf694b5
crc_cal: 246
crc_read: 246
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.5 seconds (effective 266.0 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.1 seconds (effective 341.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 455.2 kbit/s)...

Hash of data verified.
Wrote 859504 bytes (471681 compressed) at 0x00010000 in 9.1 seconds (effective 759.6 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



