*************************** START ****************************

START TIME: 202311231836

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa75c3d90
mac h: 0x96ccdb
crc_cal: 150
crc_read: 150
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 18992 bytes (13110 compressed) at 0x00001000 in 0.4 seconds (effective 384.5 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 558.4 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 746.1 kbit/s)...

Hash of data verified.
Wrote 987360 bytes (594178 compressed) at 0x00010000 in 10.8 seconds (effective 733.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202311231953

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa75c3d90
mac h: 0x96ccdb
crc_cal: 150
crc_read: 150
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 18992 bytes (13110 compressed) at 0x00001000 in 0.4 seconds (effective 383.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 543.9 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 709.9 kbit/s)...

Hash of data verified.
Wrote 987360 bytes (594178 compressed) at 0x00010000 in 10.6 seconds (effective 742.6 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



