*************************** START ****************************

START TIME: 202507222004

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xefd9a65c
mac h: 0xfdc049
crc_cal: 253
crc_read: 253
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00184020

manufacturer_id: 0x20

device_id: 0x4018

Find xmc flash and status:0x600380
flash status reg already update!

Wrote 24896 bytes (16262 compressed) at 0x00001000 in 0.5 seconds (effective 371.5 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 457.8 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 661.3 kbit/s)...

Hash of data verified.
Wrote 1230224 bytes (769086 compressed) at 0x00010000 in 12.6 seconds (effective 782.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 16 s

Download result: PASS

*************************** END ****************************



