*************************** START ****************************

START TIME: 202411081504

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xbb4db508
mac h: 0xbe2cbc
crc_cal: 190
crc_read: 190
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.4 seconds (effective 362.0 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 439.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 666.1 kbit/s)...

Hash of data verified.
Wrote 986928 bytes (609248 compressed) at 0x00010000 in 10.2 seconds (effective 771.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



