*************************** START ****************************

START TIME: 202401041742

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa75c1c1c
mac h: 0xbcccdb
crc_cal: 188
crc_read: 188
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.4 seconds (effective 361.6 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 537.2 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 723.7 kbit/s)...

Hash of data verified.
Wrote 830656 bytes (465035 compressed) at 0x00010000 in 8.7 seconds (effective 759.5 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202401041744

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa75c1c1c
mac h: 0xbcccdb
crc_cal: 188
crc_read: 188
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.4 seconds (effective 356.0 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 534.0 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 714.8 kbit/s)...

Hash of data verified.
Wrote 830656 bytes (465035 compressed) at 0x00010000 in 8.7 seconds (effective 759.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202401041818

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xa75c1c1c
mac h: 0xbcccdb
crc_cal: 188
crc_read: 188
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x00164020

manufacturer_id: 0x20

device_id: 0x4016


Wrote 17104 bytes (11191 compressed) at 0x00001000 in 0.4 seconds (effective 357.6 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 534.9 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.1 seconds (effective 726.6 kbit/s)...

Hash of data verified.
Wrote 830656 bytes (465035 compressed) at 0x00010000 in 8.8 seconds (effective 759.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 11 s

Download result: PASS

*************************** END ****************************



