Arduino Reference - StreamPeek

Arduino

Reference Language | Libraries | Comparison | Changes

## peek()

Read a byte from the file without advancing to the next one. That is, successive calls to peek() will return the same value, as will the next call to read().

This function is part of the Stream class, and is called by any class that inherits from it (Wire, Serial, etc). See the Stream class main page for more information.

#### Syntax

stream.peek()

#### Parameters

stream : an instance of a class that inherits from Stream.

#### Returns

The next byte (or character), or -1 if none is available.

#### See Also

- available()
- read()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes