nRF51 SDK: ble_bondmngr_init_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_bondmngr_init_t Struct Reference
Data Structures

Bond Manager Module init structure. This contains all options and data needed for initialization of the Bond Manager module. More...

`#include <ble_bondmngr.h>`

## Data Fields

uint8_t | flash_page_num_bond
uint8_t | flash_page_num_sys_attr
bool | bonds_delete
ble_bondmngr_evt_handler_t | evt_handler
ble_srv_error_handler_t | error_handler

## Detailed Description

Bond Manager Module init structure. This contains all options and data needed for initialization of the Bond Manager module.

## Field Documentation

bool ble_bondmngr_init_t::bonds_delete

TRUE if bonding and System Attributes for all centrals is to be deleted from flash during initialization, FALSE otherwise.

ble_srv_error_handler_t ble_bondmngr_init_t::error_handler

Function to be called in case of an error.

ble_bondmngr_evt_handler_t ble_bondmngr_init_t::evt_handler

Event handler to be called for handling events in bond manager.

uint8_t ble_bondmngr_init_t::flash_page_num_bond

Deprecated: Flash page number to use for storing Bonding Information.

uint8_t ble_bondmngr_init_t::flash_page_num_sys_attr

Deprecated: Flash page number to use for storing System Attributes.