nRF51 SDK: dm_application_param_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
dm_application_param_t Struct Reference
Device Manager Data Types

Application Registration Parameters. More...

`#include <device_manager.h>`

## Data Fields

dm_event_cb_t | evt_handler
uint8_t | service_type
ble_gap_sec_params_t | sec_param

## Detailed Description

Application Registration Parameters.

Parameters that application furnishes to the module when registering with it.

## Field Documentation

dm_event_cb_t dm_application_param_t::evt_handler

Event Handler to be registered to receive asynchronous notification from the module, see Device Manager Events for asynchronous events

uint8_t dm_application_param_t::service_type

Bit mask identifying services that the application intends to support for all peers.