nRF51 SDK: Device Manager Events

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Modules
Device Manager Events
Device Manager

This section describes the device manager events to that are notified to the application. More...

## Modules

| General Events
| General or miscellaneous events.
| Link Status Events
| Link Status Events.
| Context Management Events
| Context Management Events.

## Detailed Description

This section describes the device manager events to that are notified to the application.

Device Manager notifies the application of various asynchronous events using the asynchronous event notification callback. All events has been categorized into: a. General. b. Link Status. c. Context Management.

In the callback, these events are notified along with handle, that uniquely identifies application instance, active instance (if applicable), device instance (bonding instance, if applicable) and service instance. Not all events are pertaining to an active connection, for example a context deletion event could occur even if the peer is not connected. Also, general category of events may not be pertaining to any specific peer. See also dm_event_notification_cb and dm_application_register.