nRF51 SDK: ble_bps_s Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_bps_s Struct Reference
Blood Pressure Service

Blood Pressure Service structure. This contains various status information for the service. More...

`#include <ble_bps.h>`

## Data Fields

ble_bps_evt_handler_t | evt_handler
uint16_t | service_handle
ble_gatts_char_handles_t | meas_handles
ble_gatts_char_handles_t | feature_handles
uint16_t | conn_handle
uint16_t | feature

## Detailed Description

Blood Pressure Service structure. This contains various status information for the service.

## Field Documentation

uint16_t ble_bps_s::conn_handle

Handle of the current connection (as provided by the BLE stack, is BLE_CONN_HANDLE_INVALID if not in a connection).

ble_bps_evt_handler_t ble_bps_s::evt_handler

Event handler to be called for handling events in the Blood Pressure Service.

uint16_t ble_bps_s::feature

Value of Blood Pressure feature.

ble_gatts_char_handles_t ble_bps_s::feature_handles

Handles related to the Blood Pressure Feature characteristic.

ble_gatts_char_handles_t ble_bps_s::meas_handles

Handles related to the Blood Pressure Measurement characteristic.

uint16_t ble_bps_s::service_handle

Handle of Blood Pressure Service (as provided by the BLE stack).