nRF51 SDK: ble_gatts_rw_authorize_reply_params_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gatts_rw_authorize_reply_params_t Struct Reference
Generic Attribute Profile (GATT) Server | Structures | Generic Attribute Profile (GATT) Server

GATT Read or Write Authorize Reply parameters. More...

`#include <ble_gatts.h>`

## Data Fields

uint8_t | type
union {
ble_gatts_read_authorize_params_t read
ble_gatts_write_authorize_params_t write
} | params
union {
ble_gatts_read_authorize_params_t read
ble_gatts_write_authorize_params_t write
} | params
union {
ble_gatts_read_authorize_params_t read
ble_gatts_write_authorize_params_t write
} | params

## Detailed Description

GATT Read or Write Authorize Reply parameters.

## Field Documentation

union { ... } ble_gatts_rw_authorize_reply_params_t::params

Reply Parameters.

ble_gatts_read_authorize_params_t ble_gatts_rw_authorize_reply_params_t::read

Read authorization parameters.

uint8_t ble_gatts_rw_authorize_reply_params_t::type

Type of authorize operation, see BLE_GATTS_AUTHORIZE_TYPES.

ble_gatts_write_authorize_params_t ble_gatts_rw_authorize_reply_params_t::write

Write authorization parameters.