nRF51 SDK: ble_gatt_char_props_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gatt_char_props_t Struct Reference
Generic Attribute Profile (GATT) Common | Structures | Generic Attribute Profile (GATT) Common

GATT Characteristic Properties. More...

`#include <ble_gatt.h>`

## Data Fields

uint8_t | broadcast:1
uint8_t | read:1
uint8_t | write_wo_resp:1
uint8_t | write:1
uint8_t | notify:1
uint8_t | indicate:1
uint8_t | auth_signed_wr:1

## Detailed Description

GATT Characteristic Properties.

## Field Documentation

uint8_t ble_gatt_char_props_t::auth_signed_wr

Writing value with Signed Write Command permitted.

uint8_t ble_gatt_char_props_t::broadcast

Broadcasting of value permitted.

uint8_t ble_gatt_char_props_t::indicate

Indications of value permitted.

uint8_t ble_gatt_char_props_t::notify

Notications of value permitted.

uint8_t ble_gatt_char_props_t::read

Reading value permitted.

uint8_t ble_gatt_char_props_t::write

Writing value with Write Request permitted.

uint8_t ble_gatt_char_props_t::write_wo_resp

Writing value with Write Command permitted.