nRF51 SDK: dm_event_param_t Union Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
dm_event_param_t Union Reference
Device Manager Data Types

Event parameters. More...

`#include <device_manager.h>`

## Data Fields

ble_gap_evt_t * | p_gap_param
dm_application_context_t * | p_app_context
dm_service_context_t * | p_service_context
dm_device_context_t * | p_device_context

## Detailed Description

Event parameters.

Defines event parameters for each of the events notified by the module.

## Field Documentation

dm_application_context_t* dm_event_param_t::p_app_context

All events that are associated with application context procedures of store, load, and deletion have this as event parameter.

dm_device_context_t* dm_event_param_t::p_device_context

All events that are associated with device context procedures of store, load and deletion have this as event parameter.

ble_gap_evt_t* dm_event_param_t::p_gap_param

All events that are triggered in device manager as a result of GAP events, like connection, disconnection, security procedures are accompanied with GAP parameters.

dm_service_context_t* dm_event_param_t::p_service_context

All events that are associated with service context procedures of store, load and deletion have this as event parameter.