nRF51 SDK: ble_gatts_evt_rw_authorize_request_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gatts_evt_rw_authorize_request_t Struct Reference
Generic Attribute Profile (GATT) Server | Structures | Generic Attribute Profile (GATT) Server

Event structure for BLE_GATTS_EVT_RW_AUTHORIZE_REQUEST. More...

`#include <ble_gatts.h>`

## Data Fields

uint8_t | type
union {
ble_gatts_evt_read_t read
ble_gatts_evt_write_t write
} | request
union {
ble_gatts_evt_read_t read
ble_gatts_evt_write_t write
} | request
union {
ble_gatts_evt_read_t read
ble_gatts_evt_write_t write
} | request

## Detailed Description

Event structure for BLE_GATTS_EVT_RW_AUTHORIZE_REQUEST.

## Field Documentation

ble_gatts_evt_read_t ble_gatts_evt_rw_authorize_request_t::read

Attribute Read Parameters.

union { ... } ble_gatts_evt_rw_authorize_request_t::request

Request Parameters.

uint8_t ble_gatts_evt_rw_authorize_request_t::type

Type of authorize operation, see BLE_GATTS_AUTHORIZE_TYPES.

ble_gatts_evt_write_t ble_gatts_evt_rw_authorize_request_t::write

Attribute Write Parameters.