nRF51 SDK: bp_page17_data_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
bp_page17_data_t Struct Reference
ANT bicycle power minimum receiver example

Bicycle Power page 17 data structure. More...

`#include <bp_pages.h>`

## Data Fields

uint32_t | update_event_counter
uint32_t | wheel_ticks
uint32_t | instantaneous_cadence
uint32_t | wheel_period
uint32_t | accumulated_torgue

## Detailed Description

Bicycle Power page 17 data structure.

## Field Documentation

uint32_t bp_page17_data_t::accumulated_torgue

Accumulated torque.

uint32_t bp_page17_data_t::instantaneous_cadence

Crank cadence, if available.

uint32_t bp_page17_data_t::update_event_counter

Event counter incremented with each information update.

uint32_t bp_page17_data_t::wheel_period

Accumulated wheel period.

uint32_t bp_page17_data_t::wheel_ticks

Wheel tick count incremented with each wheel revolution.