nRF51 SDK: GATT Write operations

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GATT Write operations
Defines

## Macros

#define | BLE_GATT_OP_INVALID 0x00
#define | BLE_GATT_OP_WRITE_REQ 0x01
#define | BLE_GATT_OP_WRITE_CMD 0x02
#define | BLE_GATT_OP_SIGN_WRITE_CMD 0x03
#define | BLE_GATT_OP_PREP_WRITE_REQ 0x04
#define | BLE_GATT_OP_EXEC_WRITE_REQ 0x05

## Detailed Description

## Macro Definition Documentation

#define BLE_GATT_OP_EXEC_WRITE_REQ 0x05

Execute Write Request.

#define BLE_GATT_OP_INVALID 0x00

Invalid Operation.

#define BLE_GATT_OP_PREP_WRITE_REQ 0x04

Prepare Write Request.

#define BLE_GATT_OP_SIGN_WRITE_CMD 0x03

Signed Write Command.

#define BLE_GATT_OP_WRITE_CMD 0x02

Write Command.

#define BLE_GATT_OP_WRITE_REQ 0x01

Write Request.