nRF51 SDK: ble_version_t Struct Reference

| nRF51 SDK

- Home
- Related Pages
- API Reference
- Data Structures

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_version_t Struct Reference
Events, type definitions and API calls | Structures | Events, type definitions and API calls

Version Information. More...

`#include <ble.h>`

## Data Fields

uint8_t | version_number
uint16_t | company_id
uint16_t | subversion_number

## Detailed Description

Version Information.

## Field Documentation

uint16_t ble_version_t::company_id

Company ID, Nordic Semiconductor's company ID is 89 (0x0059) (https://www.bluetooth.org/apps/content/Default.aspx?doc_id=49708).

uint16_t ble_version_t::subversion_number

LMP Sub Version number corresponds to the SoftDevice Config ID.

uint8_t ble_version_t::version_number

LMP Version number for BT 4.0 spec is 6 (https://www.bluetooth.org/technical/assignednumbers/link_layer.htm).